|  |
| --- |
| ­­­­**Quotation** |

Service Recipient: Network Infrastructure & CCTV installation.

Visit Site: **ENG. Mahmoud / Chillout**

Visit Date: **31/03/2024.**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **No.1** | **Item** | **Vendor** | **Model** | **Description** | **Price** | **Quantity** | **Total** |
| 1 | Camera | Zero-Tech | ZTX-EG105-V2 | 1080P real-time image, high resolution, true color, Support COC AHD / TVI / CVI /CVBS standard and lossless video output CMOS progressive scan, perfectly capture the moving object, Support OSD menu High speed, long distance and real time transmission, digital WDR Auto color to B / W at low illumination Support ICR switch, true day / night, Support noise reduction function 20m IR night view distance | 695 | 5 | 3475 |
| 2 | Camera | Zero-Tech | ZTB-L5ML | Video Output Mode AHD/TVI: 5M@20fps/12.5fps, 4M@30fps/25fps/15fps, 2M@30fps/25fps; CVI: 4M@30fps/25fps, 2M@30fps/25fps Image Sensor 1/3" CMOS Sensor Image Resolution 5M:2592\*1944 4M:2560\*1440 2M:1920\*1080 Minimum Illumination Color : 0.03 lux@F2.0, AGC ON; B/W : 0 lux with IR Focus Length Fixed 3.6mm OSD , DWDR Infrared LED 42μ x 2PCS Light Distance up to 25m Housing Plastic, IP66 Operation Temperature -10℃ ~ +60℃ RH95% Max Storage Temperature -20℃ ~ +60℃ RH95% Max Power Source DC12V±10%, 450mA | 1195 | 5 | 5975 |
| 3 | Camera | Zero-Tech | ZTD-EG5MFC | 5MP @20fps/4MP real-time image, high resolution, true color AHD / TVI / CVI lossless high-definition video output, up to 1500 TVL resolution, IP67 CMOS progressive scan, perfectly capture the moving object, Lens 2.8mm Support OSD menu, Support COC High speed, long distance and real time transmission Auto color to B / W at low illumination Support ICR switch, true day / night 20 ~ 30m view distance 24/7 full color imaging | 1910 | 1 | 1910 |
| 4 | Camera | Zero-Tech | ZTB-EG5MFC | 5MP@20fps/4MP real time image, high resolution, true color AHD / TVI / CVI standard and lossless video output, Up to 1500 TVL resolution CMOS progressive scan, perfectly capture the moving object, Lens 3.6mm Support OSD menu , Support COC High speed, long distance and real time transmission Auto color to B / W at low illumination Support ICR switch, true day / night 20 ~ 30m view distance IP67 ingress protection 24/7 full color imaging Support coaxial audio transmission | 1600 | 3 | 4800 |
| 5 | Camera | Zero-Tech | ZTD-L5ML | Video Output Mode AHD/TVI: 5M@20fps/12.5fps, 4M@30fps/25fps/15fps, 2M@30fps/25fps; CVI: 4M@30fps/25fps, 2M@30fps/25fps Image Sensor 1/3" CMOS Sensor Image Resolution 5M:2592\*1944 4M:2560\*1440 2M:1920\*1080 Minimum Illumination Color : 0.03 lux@F2.0, AGC ON; B/W : 0 lux with IR Focus Length Fixed 2.8mm Infrared LED 42μ x 1PCS Infrared Distance 20M OSD , DWDR , UTC , DNR Operation Temperature -10℃~ +60℃ RH95% Max Storage Temperature -20℃ ~ +60℃ RH95% Max Power Source DC12V±10%, 500mA | 1395 | 1 | 1395 |
| 6 | DVR | Zero-Tech | ZTDXEG16CH5M | • Supports 16 CH TVI / AHD /CVI 5MP / 4MP / 1080P / 720P / WD1 video input • Supports 8 CH 5MP / 4MP / 3MP / 1080P / 960P / 720P IP video input • 8CH analog video input can be switched to 8CH IP video input • Adopt standard H.265 high profile compression format to get high-quality • Intuitive and user-friendly Graphics User Interface ( GUI ), window style • operation by mouse • Multi-mode recording: manual / timed / sensor /motion / AI recording • Playback : 16 CH simultaneously playback • Search: time slice, time, event, tag search • Express and flexible backup via USB, network and so on • Pentaplex: preview, record, playback, backup and remote access • DHCP, DDNS, PPPoE network protocol • Remote control via Web or CMS : preview, playback, backup, PTZ and • configuration • Authorization management, log review and device status review • Support 1080P output, true high resolution display • Support PTZ preset and auto cruise, up to 255 presets and 8 cruises • Support NAT function and QRCode scanning by mobile phones • Powerful mobile surveillance by smart phones with iOS and Android OS | 13000 | 1 | 13000 |
| 7 | Coaxial Cable | N/A | N/A | 300 Meter (Minimum, could need more) | 1750 | 1 | 1750 |
| 8 | Power Supply | N/A | N/A | 30 A Power Supply | 350 | 1 | 350 |
| 9 | HDD | WD | Purple | Western Digital 2TB Purple HDD | 1850 | 1 | 1850 |
| 10 | PNC | N/A | N/A | PNC | 6 | 35 | 210 |
| 11 | Power Terminal | N/A | N/A | Power Terminal | 5 | 20 | 100 |
| 12 | Workmanship (مصناعيه) | N/A | N/A | Cams Installing, Wrack Installing, DVR Configuration. | 15 | 300 | 4500 |
|  |  |  |  |  | **Total** | | 39315 |